**Derivation of Supply Curve of PV.**

Seungho Jeona, Gildong Hongb, Gyeonggi Dob,[[1]](#footnote-2)\*

a *Climate & Environment Data Center, Gyeonggi Research Institute, South Korea*

b *Climate & Environment Data Center, Gyeonggi Research Institute, South Korea*

**Abstract**

This is an abstract.

**Keywords:** Keword1, Keword-2, Keyword-3

1. Introduction

sssdfsssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssss

Sa

sssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssss

텍스트, 전자제품, 스크린샷, 웹사이트이(가) 표시된 사진

자동 생성된 설명

Fig. 1. Study Design

1. Methodology
   1. Classification of land-use and PV types

To facilitate policy design, land-use types are categorized into nine :

* 1. Exploration of PV-available sites
     1. GIS-based approach
     2. Geographical constraint

농업보호구역, 농업진흥지역, 보전산지

* 1. Calculation of PV potential

Coefficient

ssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssss

ssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssss

ssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssss

ssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssss

ssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssss

ssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssss

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| Land-use type | Area (m2) | Number of sites | PV type | Ratio (%) | Coefficient (m2/kW) | Capacity factor |
| Industrial complex | 25,293,157 | 25,128 | Roof-top PV | 59.7 | 7.23 | It is applied differently depending on the city & county to which the individual site belongs. |
| Logistics complex | 5,450,717 | 1,848 |
| Residential complex | 44,657,356 | 132,000 |
| Public buildings | 5,618,738 | 12,810 |
| Mountainous area |  |  | Ground-mounted PV |  | 11.50 |
| Farmland |  |  |
| Parking lot |  |  |
| Roadside land |  |  |
| Water | 56,372,992 | 446 | Floating PV |  |  |

텍스트, 스크린샷, 도표, 라인이(가) 표시된 사진

자동 생성된 설명

Fig. 2. Required area for PV installation in log scale. (capacity(kW) vs. area(m2))

ss

* 1. Derivation of supply curve for PV
  2. Gini coefficient

Gini

1. Results
   1. Electricity sector

Sdfsd ElecitGeographical

ssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssss

* 1. Implications for T&D networks

The last ssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssss

sssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssss

1. Conclusion

Electrification ssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssssss

**CRediT authorship contribution statement**

**Seungho Jeon:** ABC. **Gildong Hong:** ABC. **Gyeonggi Do:** ABC

**Declaration of competing interest**

The authors declare that they have no know competing financial interests or personal relationships that could have appeared to influence the work reported in this paper.

**Acknowledgement**

This work was supported by the 'Gyeonggi RE100 Platform Establishment' project through the Gyeonggi Research Institute, funded by Gyeonggi-do.

References

1. \* Corresponding author.

   *E-mail addresses:* [shjeon@gri.re.kr](mailto:shjeon@gri.re.kr) (S. Jeon), [email@gri.re.kr](mailto:email@gri.re.kr) (G. Hong), [email@gri.re.kr](mailto:email@gri.re.kr) (G. Do) [↑](#footnote-ref-2)